# Description of the 3-bit adder circuit implementation:

The solution shown is a 3-bit serial full adder. The circuit is using 6 input bits, 3 for input variable a and 3 bits for input variable b. Furthermore, 1 carry bit and 2 working bits are used.

Ein Bild, das Text, Screenshot, Schrift, Diagramm enthält.

Automatisch generierte BeschreibungIn difference to Figure 1, shown in lecture 08 – memristive in memory computing, we decided to only take two working bits into considerations. As shown in Figure 2, the implementation for a full adder algorithm for a serial computation is only using s1 and s2. Our tests have shown that nevertheless correct results were achieved.

Figure 1: serial topology memristor full adder

Ein Bild, das Text, Screenshot, Zahl, Schrift enthält.

Automatisch generierte Beschreibung

Figure 2: full adder algorithm

Ein Bild, das Text, Reihe, Schrift, Screenshot enthält.

Automatisch generierte BeschreibungFigure 3 shows the implementation in LT Spice for a 3-bit serial full adder circuit. The circuit is implemented in a serial way.

Figure : implementation 3-bit full adder

In this circuit the flow of computation is as follows: First the sum of bit a1, b1 and Carry is calculated, the result is written back to a1. Afterwards carry is newly calculated for the next iteration.

Iterations 2 and 3 are doing the exact same, except for bits a2, b2, a3 and b3.

The result is stored in a1-a3 and carry.

Following is the complete imply logic for this circuit.

s1 = 0  
s2 = 0  
a1 -> s1 = s1'  
b1 -> s2 = s2'  
s1' -> b1 = b1'  
a1 -> s2' = s2''  
a1 = 0  
b1' -> a1 = a1'  
s2'' -> a1' = a1''  
s1 = 0  
c -> s1 = s1'  
s2'' -> c = c'  
a1'' -> s1' = s1''  
a1 = 0  
s1'' -> a1 = a'  
s2 = 0  
c' -> s2 = s2'  
b1' -> s2' = s2''  
b1' -> c' = c'' first two bit added

s1 = 0  
s2 = 0  
a2 -> s1 = s1'  
b2 -> s2 = s2'  
s1' -> b2 = b2'  
a2 -> s2' = s2''  
a2 = 0  
b2' -> a2 = a2'  
s2'' -> a2' = a2''  
s1 = 0  
c -> s1 = s1'  
s2'' -> c = c'  
a2'' -> s1' = s1''  
a2 = 0  
s1'' -> a2 = a2'  
s2 = 0  
c' -> s2 = s2'  
b2' -> s2' = s2''  
b2' -> c' = c'' second two bit added

s1 = 0  
s2 = 0  
a3 -> s1 = s1'  
b3 -> s2 = s2'  
s1' -> b3 = b3'  
a3 -> s2' = s2''  
a3 = 0  
b3' -> a3 = a3'  
s2'' -> a3' = a3''  
s1 = 0  
c -> s1 = s1'  
s2'' -> c = c'  
a3'' -> s1' = s1''  
a3 = 0  
s1'' -> a3 = a3'  
s2 = 0  
c' -> s2 = s2'  
b3' -> s2' = s2''  
b3' -> c' = c'' third two bit added

final result in a1, a2, a3, c

# Input and Output

Ein Bild, das Text, Screenshot, Display, Diagramm enthält.

Automatisch generierte BeschreibungFigure 4 shows all the relevant input and output signals in the circuit for the 4 computational phases.

Figure : input Output

1. Loading data
2. Compute first stage
3. Compute second stage
4. Compute third stage

# Tests:

To check the correct behaviour of the circuit, six tests were run.

## Ein Bild, das Text, Screenshot, Display, Diagramm enthält. Automatisch generierte Beschreibung3.1 Test 1:

Figure :Test 1

Test 1 loads at the beginning following data:

a(2:0) = 3'b000

b(2:0) = 3'b111

C = 0

On the output a result of a(2:0) = 3’b111 and Cout = 0 can be observed

The result is correct.

## 3.2 Test 2

Ein Bild, das Text, Screenshot, Display, Diagramm enthält.

Automatisch generierte Beschreibung

Figure 6: Test 2

Test 2 loads at the beginning following data:

a(2:0) = 3'b100

b(2:0) = 3'b111

C = 0

On the output a result of a(2:0) = 3’b011 and Cout = 1 can be observed

The result is correct.

## 3.3 Test 3

Ein Bild, das Text, Screenshot, Diagramm, Display enthält.

Automatisch generierte Beschreibung

Figure 7: Test 3

Test 3 loads at the beginning following data:

a(2:0) = 3'b111

b(2:0) = 3'b111

C = 1

On the output a result of a(2:0) = 3’b111 and Cout = 1 can be observed

The result is correct.

## 3.4 Test 4

Ein Bild, das Text, Screenshot, Software, Diagramm enthält.

Automatisch generierte Beschreibung

Figure 8: Test 4

Test 4 loads at the beginning following data:

a(2:0) = 3'b111

b(2:0) = 3'b111

C = 0

Out = 110

Cout = 1

On the output a result of a(2:0) = 3’b110 and Cout = 1 can be observed

The result is correct.

## 3.5 Test 5

Ein Bild, das Text, Screenshot, Display, Diagramm enthält.

Automatisch generierte Beschreibung

Figure 9: Test 5

Test 5 loads at the beginning following data:

a(2:0) = 3'b100

b(2:0) = 3'b100

C = 0

Out = 110

Cout = 1

On the output a result of a(2:0) = 3’b000 and Cout = 1 can be observed

The result is correct.

## 3.6 Test 6

Ein Bild, das Text, Screenshot, Display, Diagramm enthält.

Automatisch generierte Beschreibung

Figure 10: Test 6

Test 5 loads at the beginning following data:

a(2:0) = 3'b000

b(2:0) = 3'b000

C = 0

Out = 110

Cout = 1

On the output a result of a(2:0) = 3’b000 and Cout = 0 can be observed

The result is correct.

# Summary

The tests showed that the circuit is working as accurate as expected, no failures could be found. During design of the circuit it came up that for each round of calculation the same steps need to be done. For sure this implementation can be optimised for higher speeds.

## List of illustration

[Figure 1: serial topology memristor full adder 1](#_Toc153262242)

[Figure 2: full adder algorithm 1](#_Toc153262243)

[Figure 3: implementation 3-bit full adder 2](file:///D:\Master\Emerging_Computing\epcExercise\ex04\Homework4_ECP_Bauer_Schrittwieser.docx#_Toc153262244)

[Figure 4: input Output 4](file:///D:\Master\Emerging_Computing\epcExercise\ex04\Homework4_ECP_Bauer_Schrittwieser.docx#_Toc153262245)

[Figure 5:Test 1 5](file:///D:\Master\Emerging_Computing\epcExercise\ex04\Homework4_ECP_Bauer_Schrittwieser.docx#_Toc153262246)

[Figure 6: Test 2 6](#_Toc153262247)

[Figure 7: Test 3 7](#_Toc153262248)

[Figure 8: Test 4 8](#_Toc153262249)

[Figure 9: Test 5 9](#_Toc153262250)

[Figure 10: Test 6 10](#_Toc153262251)

## Source directory

Figure 1: lecture 08 – memristive in-memory computing by Prof. Dr. Nima Taherinejad slide 24 (6.12.2024)

Figure 2: lecture 08 – memristive in-memory computing by Prof. Dr. Nima Taherinejad slide 25 (6.12.2024)

All other pictures are created by the authors.